# Electrical/Mechanical - Swellengine

**Manual Extension Sheet**

The swell engine is for all mechanical use. The electrical use is usually out of function.

To activate the electrical use please connect the magnet-coupling cables to 24VDC (or 14VDC if ordered).

Now the mechanical use is not possible anymore and the electrical function is activated.

To use the mechanical function again please disconnect the 24VDC (or 14VDC if ordered).

For the 24VDC (or 14VDC if ordered) is an additional connection-clamp installed at the outside of the swell engine.

**24V/0.63A**

**14V/1.5A**